## Phidget Capacitive Touch.lvlib:CapacitiveTouchSetDataInterval.vi

The `CapacitiveTouchDataInterval` is the time that must elapse before the channel will fire another `CapacitiveTouch_Touch` event.

- The data interval is bounded by `CapacitiveTouchMinDataInterval` and `CapacitiveTouchMaxDataInterval`.
- The timing between `CapacitiveTouch_Touch` events can also be affected by the `CapacitiveTouchTouchValueChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor: Min: 60 Max: 1000 Default: 60 1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor: Min: 60 Max: 1000 Default: 60 HIN1000_0 (ver: 104) Capacitive Touch Sensor: Min: 25 Max: 1000 Default: 25 HIN1001_0 (ver: 103, 104) Capacitive Touch Sensor: Min: 20 Max: 250 Default: 20 HIN1001_0 (ver: 103, 104) Capacitive Scroll Wheel: Min: 20 Max: 250 Default: 20

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.