## Digital Output Instrument Driver Readme

### 1. Overview

Instrument Driver Technology: LabVIEW Plug and Play (project-style)
Manufacturer: Phidgets Inc.
Supported Language(s): LabVIEW
Supported Model(s):
1010_0, 1011_0, 1012_0, 1012_1, 1012_2, 1012_3, 1013_0, 1014_0, 1014_1, 1014_2, 1014_3, 1017_0, 1017_1, 1017_2, 1018_0, 1018_1, 1018_2, 1018_3, 1019_0, 1019_1, 1023_0, 1023_1, 1024_0, 1024_1, 1030_0, 1031_0, 1032_0, 1070_0, 1072_0, 1073_0, 1202_0, 1202_1, 1202_2, 1203_0, 1203_1, 1203_2, 1219_0, 1220_0, 1221_0, 1222_0, ADP0001_0, ADP0002_0, HUB0000_0, HUB0000_1, HUB0001_0, HUB0002_0, HUB0002_1, HUB0007_0, HUB5000_0, LED1000_0, OUT1100_0, REL1000_0, REL1100_0, REL1101_0, REL1101_1, SBC3003_0
Interface(s): USB, VINT

Certified: No
NI Supported: No
Source Code Available: No

Driver Revision: 1.26.20260821
Original Release Date: 2017-06-26
Current Revision Date: 2026-08-21

### 2. Required Software

Phidget22 Core Libraries - Download Here

### 3. Revision History

Refer to Changelog for full details - Phidget22 Changelog

- 1.0.0.20170626: Initial Release
- 1.0.0.20190116: Added Failsafe Functionality. Must be paired with a version of the Phidget22 core libraries newer than the date of this release.
- 1.6.20200214: Added Frequency Functionality. Must be paired with a version of the Phidget22 core libraries newer than the date of this release.