## Phidget Temperature Sensor.lvlib:TemperatureGetTemperature.vi

The most recent temperature value that the channel has reported.

- This value will always be between `TemperatureSensorMinTemperature` and `TemperatureSensorMaxTemperature`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Temperature The temperature value Units: degrees celsius (°C) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: -70 Max: 380 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: -40 Max: 125 1045_1 (ver: 101) Temperature Sensor (IR): Min: -70 Max: 380 1045_1 (ver: 101) Temperature Sensor (IC): Min: -40 Max: 125 1048_0 (ver: 100, 101, 102) Thermocouple Input: 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: -55 Max: 150 1048_1 (ver: 200, 202, 204, 205) Thermocouple Input: 1048_1 (ver: 200, 202, 204, 205) Temperature Sensor (IC): Min: -55 Max: 150 1048_2 (ver: 210, 212, 214, 215) Thermocouple Input: 1048_2 (ver: 210, 212, 214, 215) Temperature Sensor (IC): Min: -55 Max: 150 1051_0 (ver: 100) Thermocouple Input: 1051_0 (ver: 100) Temperature Sensor (IC): Min: -55 Max: 150 1051_0 (ver: 200, 201, 202) Thermocouple Input: 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: -55 Max: 150 1051_1 (ver: 300) Thermocouple Input: 1051_1 (ver: 300) Temperature Sensor (IC): Min: -55 Max: 150 1051_2 (ver: 400, 401, 402) Thermocouple Input: 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: -55 Max: 150 DCC1000_0 (ver: 115) Temperature Sensor: Min: -40 Max: 125 DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Min: -40 Max: 125 DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Min: -40 Max: 125 DCC1020_0 (ver: 103, 104) Temperature Sensor: Min: -40 Max: 125 DCC1030_0 (ver: 104) Temperature Sensor: Min: -40 Max: 125 DCC1100_0 (ver: 113, 114) Temperature Sensor: Min: -40 Max: 125 DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Min: -40 Max: 125 DCC1100_1 (ver: 200) Temperature Sensor: Min: -40 Max: 125 DCC1120_0 (ver: 104, 105) Temperature Sensor: Min: -40 Max: 125 DCC1130_0 (ver: 105) Temperature Sensor: Min: -40 Max: 125 HUM1000_0 (ver: 104, 105) Temperature Sensor: Min: -40 Max: 85 HUM1001_0 (ver: 102) Temperature Sensor: Min: -40 Max: 85 MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Min: -40 Max: 85 MOT0110_0 (ver: 100, 104, 110, 111) Temperature Sensor: Min: -40 Max: 85 MOT0110_0 (ver: 100, 104, 110, 111) Temperature Sensor: Min: -40 Max: 85 SAF1000_0 (ver: 101, 102) Temperature Sensor: Min: -40 Max: 125 SAF1000_0 (ver: 110, 120) Temperature Sensor: Min: -40 Max: 125 TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Min: -40 Max: 85 TMP1100_0 (ver: 103, 105, 106, 108, 109, 110) Thermocouple Input: Min: -270 Max: 1370 TMP1100_0 (ver: 103, 105, 106, 108, 109, 110) Temperature Sensor (IC): Min: -40 Max: 85 TMP1101_0 (ver: 104, 106, 107, 109, 110) Thermocouple Input: Min: -270 Max: 1370 TMP1101_0 (ver: 104, 106, 107, 109, 110) Temperature Sensor (IC): Min: -40 Max: 85 TMP1101_1 (ver: 201, 202, 203, 204, 205) Thermocouple Input: Min: -270 Max: 1370 TMP1101_1 (ver: 201, 202, 203, 204, 205) Temperature Sensor (IC): Min: -40 Max: 85 TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Min: -200 Max: 850 TMP1200_1 (ver: 300, 301, 302) RTD input: Min: -200 Max: 850 TMP1202_0 (ver: 100) RTD input: Min: -200 Max: 850