## Phidget Accelerometer.lvlib:AccelerometerSetTrigger.vi

The channel will not issue a `Accelerometer_AccelerationChange` event until the acceleration value has changed by the amount specified by the `AccelerometerAccelerationChangeTrigger`.

- Setting the `AccelerometerAccelerationChangeTrigger` to 0 will result in the channel firing events every `AccelerometerDataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value Units: g-force (g) 1008_0 (ver: 101) 2-Axis Accelerometer: Min: 0 Max: 4 Default: 0 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1042_0 (ver: 300, 301, 302, 303) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1043_1 (ver: 302) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1044_0 (ver: 400, 401, 402, 403) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1044_1 (ver: 500, 502) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1044_1 (ver: 511) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 0 Max: 10 Default: 0 1053_0 (ver: 300, 301, 303) 2-Axis Accelerometer: Min: 0 Max: 10 Default: 0 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 0 Max: 10 Default: 0 1056_0 (ver: 200) 3-Axis Accelerometer: Min: 0 Max: 10 Default: 0 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Min: 0 Max: 6 Default: 0 MOT0100_0 (ver: 100, 103) 3-Axis Accelerometer: Min: 0 Max: 8 Default: 0 MOT0100_0 (ver: 100, 103) 3-Axis Accelerometer: Min: 0 Max: 8 Default: 0 MOT0109_0 (ver: 112, 113, 115, 117) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 MOT0110_0 (ver: 100, 104, 110, 111) 3-Axis Accelerometer: Min: 0 Max: 8 Default: 0 MOT0110_0 (ver: 100, 104, 110, 111) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 MOT1100_0 (ver: 201, 202) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 MOT1101_0 (ver: 112, 113) 3-Axis Accelerometer: Min: 0 Max: 16 Default: 0 MOT1102_0 (ver: 210, 212, 213) 3-Axis Accelerometer: Min: 0 Max: 8 Default: 0 MOT1102_1 (ver: 300, 301) 3-Axis Accelerometer: Min: 0 Max: 8 Default: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.