## Phidget Encoder.lvlib:EncoderGetPosition.vi

The most recent position value calculated by the Phidgets library.

- Position counts quadrature edges within a quadrature cycle. This means there are four counts per full quadrature cycle.
- Position is tracked locally as the total position change from the time the channel is opened. Setting position will only affect the local copy of the position value. This means that positions seen by multiple network applications may not agree.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Position The position value 1047_0 (ver: 100, 101, 102) Encoder Input: Default: 0 1047_1 (ver: 102, 103) Encoder Input: Default: 0 1047_2 (ver: 200) Encoder Input: Default: 0 1047_2 (ver: 301) Encoder Input: Default: 0 1052_0 (ver: 100) Encoder Input: Default: 0 1052_0 (ver: 101, 102, 103) Encoder Input: Default: 0 1052_0 (ver: 110, 111) Encoder Input: Default: 0 1057_0 (ver: 300, 301) Encoder Input: Default: 0 1057_1 (ver: 302) Encoder Input: Default: 0 1057_2 (ver: 302) Encoder Input: Default: 0 1057_3 (ver: 400, 401) Encoder Input: Default: 0 1065_0 (ver: 100, 101) Encoder Input: Default: 0 1065_1 (ver: 101) Encoder Input: Default: 0 DCC1000_0 (ver: 115) Encoder Input: Default: 0 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Default: 0 DCC1000_0 (ver: 210, 211, 220) Encoder Input: Default: 0 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Default: 0 DCC1001_0 (ver: 120, 130) Encoder Input: Default: 0 DCC1002_0 (ver: 100, 101, 102) Encoder Input: Default: 0 DCC1002_0 (ver: 111, 120) Encoder Input: Default: 0 DCC1020_0 (ver: 103, 104) Encoder Input: Default: 0 DCC1030_0 (ver: 104) Encoder Input: Default: 0 DCC1120_0 (ver: 104, 105) Encoder Input: Default: 0 DCC1130_0 (ver: 105) Encoder Input: Default: 0 ENC1000_0 (ver: 101) Encoder Input: Default: 0 ENC1001_0 (ver: 100, 101) Encoder Input: Default: 0 HIN1101_0 (ver: 101) Encoder Input: Default: 0