## Phidget Motor Position Controller.lvlib:MotorPositionControllerSetCurrentLimit.vi

The controller will limit the current through the motor to the `MotorPositionControllerCurrentLimit` value.

For more information about `MotorPositionControllerCurrentLimit`, visit our MotorPositionController API Guide

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Current Limit Motor current limit Units: amperes (A) DCC1000_0 (ver: 204, 205, 206) Position Controller: Min: 2 Max: 25 Default: 2 DCC1000_0 (ver: 210, 211, 220) Position Controller: Min: 2 Max: 25 Default: 2 DCC1001_0 (ver: 114, 116, 117) Position Controller: Min: 0 Max: 2 Default: 1 DCC1001_0 (ver: 120, 130) Position Controller: Min: 0 Max: 2 Default: 1 DCC1002_0 (ver: 100, 101, 102) Position Controller: Min: 0 Max: 3.5 Default: 1 DCC1002_0 (ver: 111, 120) Position Controller: Min: 0 Max: 4 Default: 1 DCC1020_0 (ver: 103, 104) Position Controller: Min: 5 Max: 50 Default: 5 DCC1030_0 (ver: 104) Position Controller: Min: 5 Max: 50 Default: 5 DCC1120_0 (ver: 104, 105) Position Controller: Min: 5 Max: 50 Default: 5 DCC1130_0 (ver: 105) Position Controller: Min: 5 Max: 50 Default: 5

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.