## Phidget Encoder.lvlib:EncoderSetEnabled.vi

The enabled state of the encoder.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Enabled The enabled value 1047_0 (ver: 100, 101, 102) Encoder Input: Default: 1 1047_1 (ver: 102, 103) Encoder Input: Default: 1 1047_2 (ver: 200) Encoder Input: Default: 1 1047_2 (ver: 301) Encoder Input: Default: 1 1052_0 (ver: 100) Encoder Input: Default: 1 1052_0 (ver: 101, 102, 103) Encoder Input: Default: 1 1052_0 (ver: 110, 111) Encoder Input: Default: 1 1057_0 (ver: 300, 301) Encoder Input: Default: 1 1057_1 (ver: 302) Encoder Input: Default: 1 1057_2 (ver: 302) Encoder Input: Default: 1 1057_3 (ver: 400, 401) Encoder Input: Default: 1 1065_0 (ver: 100, 101) Encoder Input: Default: 1 1065_1 (ver: 101) Encoder Input: Default: 1 DCC1000_0 (ver: 115) Encoder Input: Default: 1 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Default: 1 DCC1000_0 (ver: 210, 211, 220) Encoder Input: Default: 1 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Default: 1 DCC1001_0 (ver: 120, 130) Encoder Input: Default: 1 DCC1002_0 (ver: 100, 101, 102) Encoder Input: Default: 1 DCC1002_0 (ver: 111, 120) Encoder Input: Default: 1 ENC1000_0 (ver: 101) Encoder Input: Default: 1 ENC1001_0 (ver: 100, 101) Encoder Input: Default: 1 HIN1101_0 (ver: 101) Encoder Input: Default: 1

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.