## Phidget Voltage Output.lvlib:VoltageOutputSetVoltageOutputRange.vi

Choose a `VoltageOutputVoltageOutputRange` that best suits your application.

- Changing the `VoltageOutputVoltageOutputRange` will also affect the `VoltageOutputMinVoltage` and `VoltageOutputMaxVoltage` values.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage Output Range The output range value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1002_0 v100 v101 | OUT1001_0 v103 | OUT1001_0 v110 v111 v120 | OUT1002_0 v100 | OUT1002_0 v110 v111 v120
VOLTAGE_OUTPUT_RANGE_10V | 1 | ✓ | ✓ | ✓ | ✓ | ✓
VOLTAGE_OUTPUT_RANGE_5V | 2 | X | ✓ | ✓ | ✓ | ✓
1002_0 (ver: 100, 101) Voltage Output: Default: VOLTAGE_OUTPUT_RANGE_10V OUT1001_0 (ver: 103) Voltage Output: Default: VOLTAGE_OUTPUT_RANGE_10V OUT1001_0 (ver: 110, 111, 120) Voltage Output: Default: VOLTAGE_OUTPUT_RANGE_10V OUT1002_0 (ver: 100) Voltage Output: Default: VOLTAGE_OUTPUT_RANGE_10V OUT1002_0 (ver: 110, 111, 120) Voltage Output: Default: VOLTAGE_OUTPUT_RANGE_10V

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.