## Phidget Capacitive Touch.lvlib:CapacitiveTouchGetIsTouched.vi

The most recent touch state that the channel has reported.

- This will be 0 or 1

- 0 is not touched
- 1 is touched

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Touched The touched state 1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor: 1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor: HIN1000_0 (ver: 104) Capacitive Touch Sensor: HIN1001_0 (ver: 103, 104) Capacitive Touch Sensor: HIN1001_0 (ver: 103, 104) Capacitive Scroll Wheel: