Data Adapter Settings

Voltage | Baud rate
Chip Select Mode | SPI Mode | Endianess

Send Data

Data (in bytes) |  | Wait for response?

Send and Receive Data

Device Address (in bytes) |
Data (in bytes) |
Number of bytes to read |

Complex Transaction

Device Address (in bytes) |
Packet Format |  | See API for details on packet format
Data (in bytes) |

Communication

Time | Sent | Received

Errors

Time | Error # | Desc |
--- | --- | --- | ---