## Phidget Data Adapter.lvlib:DataAdapterSetDataAdapterVoltage.vi

The voltage used to communicate with and power the external device.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage The voltage value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
ADP0001_0 v200 v201 | ADP0001_0 v200 v201 | ADP0002_0 v100 | ADP0002_0 v100
DATAADAPTER_VOLTAGE_EXTERN | 1 | ✓ | ✓ | ✓ | ✓
DATAADAPTER_VOLTAGE_2_5V | 3 | ✓ | ✓ | ✓ | ✓
DATAADAPTER_VOLTAGE_3_3V | 4 | ✓ | ✓ | ✓ | ✓
DATAADAPTER_VOLTAGE_5_0V | 5 | ✓ | ✓ | ✓ | ✓
ADP0001_0 (ver: 200, 201) Data Adapter: Default: DATAADAPTER_VOLTAGE_EXTERN ADP0001_0 (ver: 200, 201) Data Adapter: Default: DATAADAPTER_VOLTAGE_EXTERN ADP0002_0 (ver: 100) Data Adapter: Default: DATAADAPTER_VOLTAGE_EXTERN ADP0002_0 (ver: 100) Data Adapter: Default: DATAADAPTER_VOLTAGE_EXTERN

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.