## Phidget RFID.lvlib:RFIDSetAntennaEnabled.vi

The on/off state of the antenna.

- You can turn the antenna off to save power.
- You must turn the antenna on in order to detect and read RFID tags.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Antenna Enabled The state of the antenna 1023_0 (ver: 103) RFID Reader: Default: 1 1023_0 (ver: 104) RFID Reader: Default: 1 1023_0 (ver: 200) RFID Reader: Default: 1 1023_0 (ver: 201, 202, 203, 204) RFID Reader: Default: 1 1023_1 (ver: 205, 206) RFID Reader: Default: 1 1024_0 (ver: 100, 101, 103) RFID Reader/Writer: Default: 1 1024_1 (ver: 301) RFID Reader/Writer: Default: 1 1024_1 (ver: 301) RFID Reader/Writer: Default: 1 1024_1 (ver: 310) RFID Reader/Writer: Default: 1 1024_1 (ver: 310) RFID Reader/Writer: Default: 1 1024_1 (ver: 320) RFID Reader/Writer: Default: 1 1024_1 (ver: 320) RFID Reader/Writer: Default: 1

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.