## Phidget Frequency Counter.lvlib:FrequencyCounterSetFilterType.vi

Determines the signal type that the channel responds to.

- The filter type is chosen based on the type of input signal. See the `FrequencyFilterType` entry under Enumerations for more information.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Filter Type The filter value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1054_0 v100 v101 | DAQ1400_0 v112 | DAQ1400_0 v120 v121 | DAQ1400_0 v130 v131
FILTER_TYPE_ZERO_CROSSING | 1 | ✓ | X | X | X
FILTER_TYPE_LOGIC_LEVEL | 2 | ✓ | ✓ | ✓ | ✓
1054_0 (ver: 100, 101) Frequency Input: Default: FILTER_TYPE_LOGIC_LEVEL DAQ1400_0 (ver: 112) Frequency Input: Default: FILTER_TYPE_LOGIC_LEVEL DAQ1400_0 (ver: 120, 121) Frequency Input: Default: FILTER_TYPE_LOGIC_LEVEL DAQ1400_0 (ver: 130, 131) Frequency Input: Default: FILTER_TYPE_LOGIC_LEVEL

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.